| DRIVER'S DOOR WIRING
H45/DG

#### 203
DRIVER'S WINDOW MOTOR
RET03/LVILVE/NINAV4/RAD03,RAD07

5 | 1.2 | 21E | ONE-TOUCH ELECTRIC WINDOW NORMAL DOWN - CONTROL | ?????
7 | 1.2 | 21C | ONE-TOUCH ELECTRIC WINDOW NORMAL UP - CONTROL | ?????
9 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
11 | 1.2 | 21AA | DRIVER ELECTRIC WINDOW RAISE/LOWER CONTROL | ?????
13 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | C426E
14 | 1.2 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | C426E