| DRIVER'S DOOR WIRING
H45/DG

#### 132
DRIVER'S SIDE ELECTRIC WINDOW CONTROL
RET03/LVILVE/NINAV4/RAD03,RAD07

2 | 1.2 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
4 | 1.2 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
5 | 1.2 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
6 | 1.2 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
7 | 1.2 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
9 | 1.2 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL | ?????
10 | 1.2 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL | ?????
12 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
13 | 1.2 | 21E | ONE-TOUCH ELECTRIC WINDOW NORMAL DOWN - CONTROL | ?????
14 | 1.2 | 21AA | DRIVER ELECTRIC WINDOW RAISE/LOWER CONTROL | ?????
15 | 1.2 | 21C | ONE-TOUCH ELECTRIC WINDOW NORMAL UP - CONTROL | ?????