| CONNECTION
ANY TYPE

#### R38
DASHBOARD/LEFT-HAND ROOF CONNECTION
H45 DG/ALEVA/RETRCR/NINAV4/RAD04,RAD05,RAD07

3 | 0.5 | BP6 | PROTECTED + BATTERY FEED > INTERIOR LIGHT | M049
6 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | M049
11 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | M049
12 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | M049
13 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M049
14 | 0.5 | 107J | TELEPHONE MICROPHONE SCREENING | M049
15 | 0.5 | 107F | MULTIMEDIA MICROPHONE SIGNAL | M049
16 | 0.5 | 107G | HANDS FREE TELEPHONE MICROPHONE + | M049
18 | 0.5 | 14S | RAIN SENSOR SERIAL LINE SIGNAL | M049