| ENGINE WIRING
2TR/BVVR

#### 119
AUTOMATIC TRANSMISSION COMPUTER
CA01,CA02/2TR703

A1 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
B1 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
C1 | 0.5 | 5NT | PRIMARY SPEED SENSOR SIGNAL 1 | ?????
D1 | 0.5 | 5PR | SECONDARY SPEED SENSOR SIGNAL | ?????
G1 | 0.5 | 5HG | LOCKING ON/OFF SELECTION SOLENOID VALVE CONTROL | ?????
H1 | 0.5 | 5DL | MODULATING SOLENOID VALVE 3 | ?????
J1 | 0.5 | 5R | MODULATING SOLENOID VALVE 2 | ?????
K1 | 0.5 | 5Q | MODULATING SOLENOID VALVE 1 | ?????
L1 | 0.5 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER | ?????
M1 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | ?????
E2 | 0.5 | 5HN | SENSOR EARTH | ?????
F2 | 0.5 | 5HX | + SENSOR FEED | ?????
G2 | 0.5 | 5HM | STEPPER MOTOR COIL D CONTROL | ?????
H2 | 0.5 | 5HL | STEPPER MOTOR COIL C CONTROL | ?????
J2 | 0.5 | 5HK | STEPPER MOTOR COIL B CONTROL | ?????
K2 | 0.5 | 5HH | STEPPER MOTOR COIL A CONTROL | ?????
L2 | 0.5 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER | ?????
M2 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | ?????
A3 | 0.5 | 5DF | MULTIFUNCTION SWITCH SIGNAL 1 | ?????
C3 | 0.5 | 5BZ | GEARBOX OIL TEMPERATURE + | ?????
D3 | 0.5 | 5HW | PRIMARY PRESSURE SENSOR SIGNAL (PRIMARY PULLEY) | ?????
E3 | 0.5 | 5HU | SECONDARY PRESSURE SENSOR SIGNAL (SECONDARY PULLEY) | ?????
A4 | 0.5 | H66P | REVERSING LIGHTS + CONTROL | ?????
B4 | 0.5 | 5DH | MULTIFUNCTION SWITCH SIGNAL 3 | ?????
C4 | 0.5 | 5DJ | MULTIFUNCTION SWITCH SIGNAL 4 | ?????
D4 | 0.5 | 5KN | GEAR LEVER SWITCH 1 SIGNAL | ?????
E4 | 0.5 | NUH | FRONT RIGHT-HAND SIDE MEMBER ELECTRONIC EARTH | ?????
G4 | 0.5 | 5HNA | EARTH SENSOR 2 | ?????
H4 | 0.5 | 5HP | CVT COMPUTER CLOCK SIGNAL | ?????
J4 | 0.5 | 5HQ | REPROGRAMMABLE MEMORY SELECTION SIGNAL | ?????
K4 | 0.5 | 5HR | INPUT/OUTPUT DATA SIGNAL | ?????
M4 | 0.5 | NUH | FRONT RIGHT-HAND SIDE MEMBER ELECTRONIC EARTH | ?????