| DASHBOARD WIRING
H45/DG

#### 878
LH MIXER MOTOR
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD03/BVA6/BVVR

1 | 0.3 | 38SQ | LEFT-HAND MIXER MOTOR B2 COIL CONTROL | F001
2 | 0.3 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | F001
3 | 0.3 | 38SS | LEFT-HAND MIXER MOTOR B1 COIL CONTROL | F001
4 | 0.3 | 38SR | LEFT-HAND MIXER MOTOR A2 COIL CONTROL | F001
6 | 0.3 | 38ST | LEFT-HAND MIXER MOTOR A1 COIL CONTROL | F001