| RIGHT-HAND REAR WIRING
H45/DG

#### 261
RADIO
TR4X4/RAD03

1 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
2 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
3 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
15 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
17 | 0.5 | 34HK | - INFRARED REMOTE CONTROL | ?????
18 | 0.5 | 34HL | + INFRARED REMOTE CONTROL | ?????
19 | 0.5 | 34HU | MULTIMEDIA WAKE-UP SIGNAL | ?????