| LEFT-HAND REAR DOOR WIRING
H45

#### 131
REAR LEFT-HAND ELECTRIC WINDOW CONTROL
DG/LVILVI/RAD04,RAD05

1 | 1.2 | 21ZB | WINDOW WINDER THERMAL PROTECTION SIGNAL | ?????
2 | 1.2 | 23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN | ?????
3 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
4 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
7 | 1.2 | 23BA | REAR LEFT-HAND ELECTRIC WINDOW RAISE/LOWER CONTROL | ?????
8 | 1.2 | 23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE | ?????