| RIGHT-HAND REAR WIRING
H45/DD

#### 1175
ESP SENSOR AND TRANSVERSE AND LATERAL ACCELERATION
TR4X4,TR4X2/RAD03

2 | 0.5 | 4CY | YAW SENSOR - (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | F045E
4 | 0.5 | 4CZ | YAW SENSOR + (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | F045E
5 | 0.5 | 4CZA | CLUSTER SENSOR SERIES CONNECTION + SIGNAL | F045E
6 | 0.5 | 4CZB | CLUSTER SENSOR SERIES CONNECTION - SIGNAL | F045E