| CONNECTION
ANY TYPE

#### R456
DRIVER'S DOOR WIRING/DASHBOARD WIRING CONNECTION 2
H45/DG FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD05/BVM6

4 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
5 | 1.2 | 21ZA | WINDOW WINDER THERMAL PROTECTION SIGNAL 1 | ?????
9 | 0.5 | 20DC | DRIVER'S DOOR LOCKING SIGNAL | ?????
10 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
11 | 1.2 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL | ?????
12 | 1.2 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????