| CONNECTION
ANY TYPE

#### R462
PEDALS/DASHBOARD 2
H45/BVA6/M9R DG/TR4X4/SSESP/NINAV4/RAD04,RAD05,RAD07

1 | 0.3 | 3PD | SPEED LIMITER ON/OFF CONTROL | ?????
3 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL | ?????
4 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY) | ?????
7 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | ?????
9 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1 | ?????
10 | 0.5 | 86M | CRUISE CONTROL PROGRAMMING RETURN SIGNAL | ?????
11 | 0.3 | 3FX | CRUISE CONTROL ON>OFF - CONTROL | ?????
12 | 0.5 | 86G | CRUISE CONTROL PROGRAMMING CONTROL | ?????
13 | 0.5 | 4DS | - YAW SENSOR | ?????
14 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY) | ?????
16 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | ?????
17 | 0.5 | AP1C | PROTECTED + AFTER IGNITION FEED/4X4 COMPUTER | ?????
19 | 0.5 | 115A | OIL TEMPERATURE SENSOR - SIGNAL | ?????
20 | 0.5 | HK | DIAGNOSTIC SIGNAL K | ?????