243414M462
1	0.5	LP	PROTECTED + SIDE LIGHT FEED	M004
2	0.5	CPD	PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT +	M004
3	0.5	CANH	DIAGNOSTIC CAN H SIGNAL 	M004
4	0.3	26LC	COLUMN STATUS SIGNAL 2	M004
6	0.5	38EW	0 VOLT EVAPORATOR TEMPERATURE SENSOR CLIMATE CONTROL SIGNAL	M004
7	0.5	30A	BRAKE FLUID LEVEL WARNING LIGHT - CONTROL	M004
8	0.3	65Q	STOP SWITCH SIGNAL 2	M004
9	0.5	60JG	FRONT FRONTAL SATELLITE - SIGNAL	M004
10	0.5	11S	RIGHT-HAND PROTECTED SIDE LIGHT +CONTROL	M004
11	0.5	11T	LEFT-HAND PROTECTED SIDE LIGHT +CONTROL	M004
12	0.5	CPG	PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT +	M004
13	0.5	CANL	DIAGNOSTIC CAN L SIGNAL 	M004
14	0.3	26Z	AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL	M004
15	0.3	26LB	COLUMN STATUS SIGNAL 1	M004
16	0.5	3B	AIR TEMPERATURE SENSOR + SIGNAL	M004
17	0.5	26BM	OIL PRESSURE WARNING LIGHT/ALTERNATOR CHARGING INDICATOR LIGHT CONTROL	M004
18	0.5	H66P	REVERSING LIGHTS + CONTROL	M004
19	0.5	NV	FRONT LEFT-HAND SIDE MEMBER ELECTRONIC EARTH 3	M004
20	0.5	60JF	FRONT FRONTAL SATELLITE + SIGNAL	M004
