| CONNECTION
ANY TYPE

#### R1
DASHBOARD/RIGHT REAR CONNECTION
H45/DD FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/RAD03/BVM6

2 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | F010
3 | 1.2 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
6 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
7 | 1.2 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
8 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
9 | 1.2 | 3N | FUEL PUMP + | ?????
12 | 0.85 | BP26 | CARPHONE PROTECTED + BATTERY FEED | F010
13 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
14 | 0.5 | 64D | RIGHT HAND TURN SIGNAL LIGHTS CONTROL | ?????
15 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
16 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
17 | 1.2 | 79A | HEATED SEAT + CONTROL | ?????
19 | 3.0 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL | ?????