| FRONT WIRING
H45/BVVR/2TR

#### 227
LEFT-HAND HEADLIGHT
DD/TR4X4/SSESP/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 0.5 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
2 | 0.5 | 11T | LEFT-HAND PROTECTED SIDE LIGHT +CONTROL | ?????
4 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
5 | 0.85 | CPG | PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT + | ?????
6 | 0.85 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
7 | 0.85 | RPG | LEFT HAND PROTECTED MAIN BEAM HEADLIGHT + | ?????
8 | 0.85 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????