| RIGHT-HAND REAR WIRING
H45/DG

#### 261
RADIO
TR4X4/RAD07

1 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
2 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
3 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
11 | 0.5 | TB26 | TELEPHONE VOICE SHIELDED CABLE | ?????
12 | 0.5 | 107M | TELEPHONE AUDIO - SIGNAL | ?????
15 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
18 | 0.5 | 107E | RADIO SOUND CUT-OFF SIGNAL FOR TELEPHONE | ?????
19 | 0.5 | 34HU | MULTIMEDIA WAKE-UP SIGNAL | ?????
24 | 0.5 | 107L | TELEPHONE AUDIO + SIGNAL | ?????