24341AR422
1	0.5	87T	BOOT LID POSITION SWITCH 1 SIGNAL	?????
2	1.2	A1	+ AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY	?????
3	1.2	36A	REAR WIPER + CONTROL	?????
5	0.85	20S	TAILGATE MOTOR OPENING AUTHORISED FEED	?????
6	1.2	BP48	PROTECTED + BATTERY FEED > ELECTRIC WINDOW	?????
8	0.85	H66P	REVERSING LIGHTS + CONTROL	?????
9	0.5	36C	REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL	?????
