| CONNECTION
ANY TYPE

#### R462
PEDALS/DASHBOARD 2
H45/BVVR/2TR DG/TR4X2/SSESP/NINAV4/RAD04,RAD05,RAD07

1 | 0.3 | 3PD | SPEED LIMITER ON/OFF CONTROL | ?????
9 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1 | ?????
10 | 0.5 | 86M | CRUISE CONTROL PROGRAMMING RETURN SIGNAL | ?????
11 | 0.3 | 3FX | CRUISE CONTROL ON>OFF - CONTROL | ?????
12 | 0.5 | 86G | CRUISE CONTROL PROGRAMMING CONTROL | ?????
19 | 0.5 | 115A | OIL TEMPERATURE SENSOR - SIGNAL | ?????
20 | 0.5 | HK | DIAGNOSTIC SIGNAL K | ?????