| FRONT WIRING
H45/BVA6/M9R

#### 1067
ADDITIONAL HEATING RELAY 1
DD/TR4X4/ASRES2/LADECH/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 3.0 | BP9 | PROTECTED + BATTERY FEED ADDITIONAL HEATER FUSE | ?????
2 | 0.5 | 38JU | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 1 | ?????
3 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
4 | 3.0 | 38LL | PASSENGER COMPARTMENT HEATING RESISTANCE / RELAY 1 CONTROL | ?????