| ENGINE WIRING
M9R/BVM6

#### 120
INJECTION COMPUTER
TR4X4/CA01,CA02/M9R830,M9R832

B1 | 0.5 | 3AAZ | WATER PUMP RELAY/FUEL PRESSURE ADJUSTMENT- CONTROL | ?????
H1 | 0.5 | 3DV | AIRFLOW SENSOR + SIGNAL | ?????
J1 | 0.5 | 3ABQ | AIR FLOW TEMPERATURE SIGNAL | ?????
L1 | 0.5 | 3AAX | + SWIRL FLAP MOTOR + CONTROL | ?????
M1 | 0.5 | 3VQ | CONTROL - GAS RECIRCULATION MOTOR | ?????
C2 | 1.2 | 3KG | INLET FLAP SOLENOID VALVE - CONTROL | ?????
D2 | 0.5 | 3FF | PRE-HEATER RELAY - CONTROL | ?????
G2 | 0.5 | 38KQ | +AIR VENT POSITION SENSOR | ?????
J2 | 0.5 | 38KS | RIGHT-HAND AIR VENT POSITION SIGNAL | ?????
K2 | 0.5 | 3DW | AIRFLOW SENSOR - SIGNAL | ?????
L2 | 0.5 | 3AAY | -SWIRL FLAP MOTOR - CONTROL | ?????
M2 | 0.5 | 3VP | CONTROL + GAS RECIRCULATION MOTOR | ?????
A3 | 0.5 | 3BL | ENGINE SPEED > TDC SENSOR - SIGNAL | ?????
D3 | 0.5 | 3AA | INJECTION LOCKING RELAY COIL - CONTROL | ?????
H3 | 0.5 | 3AAV | -UPSTREAM DIESEL OXYGEN SENSOR | ?????
J3 | 0.5 | 3AAW | DOWNSTREAM DIESEL OXYGEN SENSOR HUNTING CURRENT SIGNAL | ?????
L3 | 0.5 | 3RG | PRESSURE RAIL (COMMON RAIL) CONTROL- ADJUSTMENT | ?????
M3 | 2.0 | 3FB1 | INJECTION + > PROTECTIVE RELAY | ?????
A4 | 0.5 | 3BG | ENGINE SPEED SIGNAL > TDC SENSOR | ?????
B4 | 0.5 | 3FY | PRE-HEATER RELAY DIAGNOSTIC SIGNAL | ?????
C4 | 0.5 | 3MG | TURBO PRESSURE SOLENOID VALVE - CONTROL | ?????
H4 | 0.5 | 3AAT | UPSTREAM DIESEL OXYGEN SENSOR OUTPUT VOLTAGE | ?????
J4 | 0.5 | 3AAU | UPSTREAM DIESEL OXYGEN SENSOR COMPENSATION RESISTOR SIGNAL | ?????
K4 | 0.5 | 38KP | -AIR VENT POSITION SENSOR | ?????
L4 | 0.5 | 3HI | FUEL PRESSURE CONTROL SOLENOID VALVE - CONTROL | ?????
M4 | 2.0 | 3FB2 | INJECTION + > PROTECTIVE RELAY | ?????