| FRONT PASSENGER DOOR WIRING
H45/DG

#### 133
PASSENGER'S SIDE ELECTRIC WINDOW CONTROL
RET02,RET03/LVILVE/NINAV1/RAD01,RAD02,RAD04,RAD05

2 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
4 | 1.2 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL | ?????
5 | 1.2 | 22U | PASSENGER'S ELECTRIC WINDOW UP CONTROL | ?????
6 | 1.2 | 22V | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL | ?????
7 | 1.2 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL | ?????
8 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????