8200147803
E2	0.5	CANH	DIAGNOSTIC CAN H SIGNAL 	?????
F2	0.5	26Z	AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL	?????
G2	0.5	65A	BRAKE LIGHTS + CONTROL	?????
H2	0.5	65Q	STOP SWITCH SIGNAL 2	?????
A3	0.5	3LR	+ LOAD POTENTIOMETER 1	?????
B3	0.5	3LU	+ LOAD POTENTIOMETER 2 	?????
C3	0.5	3NAA	+5V TANK PRESSURE SENSOR	?????
D3	0.5	3NAB	TANK PRESSURE SENSOR SIGNAL	?????
E3	0.3	3PD	SPEED LIMITER ON/OFF CONTROL 	?????
F3	0.3	3FX	CRUISE CONTROL ON>OFF - CONTROL	?????
G3	1.2	MZR	FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT	?????
H3	1.2	MZR	FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT	?????
A4	0.5	3LV	- LOAD POTENTIOMETER 2 	?????
B4	0.5	HK	DIAGNOSTIC SIGNAL K	?????
C4	0.5	86M	CRUISE CONTROL PROGRAMMING RETURN SIGNAL 	?????
D4	0.5	3NAD	FUEL TEMPERATURE/TANK PRESSURE - SENSOR	?????
E4	0.5	3LT	- LOAD POTENTIOMETER 1 	?????
F4	0.5	41B	FUEL LEVEL  -	?????
G4	1.2	MZR	FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT	?????
H4	1.2	MZR	FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT	?????
A1	0.5	3LS	LOAD POTENTIOMETER 1 + SIGNAL	?????
B1	0.5	86G	CRUISE CONTROL PROGRAMMING CONTROL 	?????
D1	0.85	AP17	PROTECTED + AFTER IGNITION, INJECTION SIMULATOR FUSE	?????
E1	0.5	CANL	DIAGNOSTIC CAN L SIGNAL 	?????
G1	1.2	3FB	INJECTION + > PROTECTIVE RELAY	?????
H1	1.2	3M	CANISTER BLEED SOLENOID VALVE - CONTROL (PETROL VAPOUR ABSORBER)	?????
A2	0.5	3LW	LOAD POTENTIOMETER 2 + SIGNAL	?????
B2	0.5	3NAB	TANK PRESSURE SENSOR SIGNAL	?????
